sua_ser

Configure an Internal Server Behind SUA

- Introduction

If you wish, you can make internal servers (e.g., Web, ftp or mail server) accessible for outside users, even though SUA makes your LAN appear as a single machine to the outside world. A service is identified by the port number. Also, since you need to specify the IP address of a server in the Prestige, a server must have a fixed IP address and not be a DHCP client whose IP address potentially changes each time it is powered on.

In addition to the servers for specific services, SUA supports a default server. A service request that does not have a server explicitly designated for it is forwarded to the default server. If the default server is not defined, the service request is simply discarded.

- Configuration

To make a server visible to the outside world, specify the port number of the service and the inside address of the server in 'Menu 15.2.1', Multiple Server Configuration. The outside users can access the local server using the Prestige's WAN IP address which can be obtained from menu 24.1.

- For example (Configuring an internal Web server for outside access) :

  `Menu 15.2.1 - NAT Server Setup (Used for SUA Only)
  Rule Start Port No. End Port No. IP Address
  ---------------------------------------------------
  1. Default Default 0.0.0.0
  2. 80 80 192.168.1.10
  3. 0 0 0.0.0.0
  4. 0 0 0.0.0.0
  5. 0 0 0.0.0.0
  6. 0 0 0.0.0.0
  7. 0 0 0.0.0.0
  8. 0 0 0.0.0.0
  9. 0 0 0.0.0.0
  10. 0 0 0.0.0.0
  11. 0 0 0.0.0.0
  12. 0 0 0.0.0.0`

  `Press ENTER to Confirm or ESC to Cancel:
  `

- Port numbers for some services

Service | Port Number
FTP | 21
Telnet | 23
SMTP | 25
DNS (Domain Name Server) | 53
www-http (Web) | 80

All contents copyright © 2002 ZyXEL Communications Corporation.