ZyXEL TFTP Support

Firmware/Configurations Uploading and Downloading using TFTP

- Using TFTP client software
- Using TFTP command on Windows NT
- Using TFTP command on UNIX
- Downloading Walusoft TFTP from http://www.walusoft.co.uk

- Using TFTP client software

- Upload/download ZyNOS via LAN
- Upload/download SMT configurations via LAN

Using TFTP to upload/download ZyNOS via LAN

- TELNET to your Prestige first before running the TFTP software
- Type the CI command 'sys stdio 0' to disable console idle timeout in Menu 24.8 and stay in Menu 24.8
- Run the TFTP client software
- Enter the IP address of the Prestige
- To upload the firmware, please save the remote file as 'ras' to Prestige. After the transfer is complete, the Prestige will program the upgraded firmware into FLASH ROM and reboot itself.
- To download the firmware, please get the remote file 'ras' from the Prestige.

> > An example:

The 192.168.1.1 is the IP address of the Prestige. The local file is the source file of the ZyNOS firmware that is available in your hard disk. The remote file is the file name that will be saved in Prestige. Check the port number 69 and 512-Octet blocks for TFTP. Check 'Binary' mode for file transfering.

Using TFTP to upload/download SMT configurations via LAN

- TELNET to your Prestige first before running the TFTP software
- Type the CI command 'sys stdio 0' to disable console idle timeout in Menu 24.8 and stay in Menu 24.8
- Run the TFTP client software
- To download the SMT configuration, please get the remote file 'rom-0' from the Prestige.
- To upload the SMT configuration, please save the remote file as 'rom-0' in the Prestige.

> > An Example:

- The 192.168.1.1 is the IP address of the Prestige.
- The local file is the source file of your configuration file that is available in your hard disk.
- The remote file is the file name that will be saved in Prestige.
- Check the port number 69 and 512-Octet blocks for TFTP.
- Check 'Binary' mode for file transfering.

- Using TFTP command on Windows NT

Before you begin:

1. TELNET to your Prestige first before using TFTP command
2. Type the CI command 'sys stdio 0' to disable console idle timeout in Menu 24.8 and stay in Menu 24.8

- Upload ZyNOS via LAN

`c:\tftp -i [PrestigeIP] put [localfile] ras`

- Download ZyNOS via LAN

`c:\tftp -i [PrestigeIP] get ras [localfile]`

- Upload SMT configurations via LAN

`c:\tftp -i [PrestigeIP] put [localfile] rom-0`

- Download SMT configurations via LAN

`c:\tftp -i [PrestigeIP] get rom-0 [localfile]`

- Using TFTP command on UNIX

Before you begin:

1. TELNET to your Prestige first before using TFTP command
2. Type the CI command 'sys stdio 0' to disable console idle timeout in Menu 24.8 and stay in Menu 24.8

Example:

`[cppwu@faelinux cppwu]$ telnet 192.168.1.1`
`Trying 192.168.1.1...`
`Connected to 192.168.1.1.`
`Escape character is '^]'.`

`Password: ****`

`Copyright (c) 1994 - 1999 ZyXEL Communications Corp.`

`Prestige 642 Main Menu`

`Getting Started Advanced Management`
`1. General Setup 21. Filter Set Configuration`
`3. Ethernet Setup 22. SNMP Configuration`
`4. Internet Access Setup 23. System Password`
`24. System Maintenance`

`Advanced Applications`
`11. Remote Node Setup`
`12. Static Routing Setup`
`15. SUA Server Setup 99. Exit`

`Enter Menu Selection Number: 24`

`Menu 24 - System Maintenance`

`1. System Status`
`2. System Information and Console Port Speed`
`3. Log and Trace`
`4. Diagnostic`
`5. Backup Configuration`
`6. Restore Configuration`
`7. Firmware Update`
`8. Command Interpreter Mode`

`Copyright (c) 1999 ZyXEL Communications Corp.n Number: 8`
`ras> sys stdio 0`
`ras> (press Ctrl+] to escape to Telnet prompt)`
`telnet> z`
`[1]+ Stopped telnet 192.168.1.1`
`[cppwu@faelinux cppwu]$ tftp`
`tftp> connect 192.168.1.1`
`tftp> binary <- change to binary mode`
`tftp> get rom-0 [local-rom] <- download configurations`
`tftp> get ras [local-firmware] <- download firmware`
`tftp> put [local-rom] rom-0 <- upload configurations`
`tftp> put [local-firmware] ras <- upload firmware`

> All contents copyright (c) 2000 ZyXEL Communications Corporation.